|  |  |  |
| --- | --- | --- |
| Catalog of products | FFC/FPC connectors |  |
| Spacing | 0.5mm |  |
| Number of contacts | 40 |  |
| Locking characteristic | Clamshell type |  |
| Installation Type | Lying down tape |  |
| Type of contact | Down connection |  |
| Height on board | 2mm |  |
| Access flexible cable thickness | 0.3mm |  |
| Operating temperature range | -25℃~+85℃ |  |

